Name – Sujit Dhage Roll NO.=B43007

EXP 2 4-BIT ALU

ibrary IEEE;

use IEEE.STD\_LOGIC\_1164.ALL;

use IEEE.STD\_LOGIC\_unsigned.ALL; use IEEE.STD\_LOGIC\_arith.ALL;

-- Uncomment the following library declaration if using

-- arithmetic functions with Signed or Unsigned values

--use IEEE.NUMERIC\_STD.ALL;

-- Uncomment the following library declaration if instantiating

-- any Xilinx primitives in this code.

--library UNISIM;

--use UNISIM.VComponents.all; entity abc is

Port ( a : in STD\_LOGIC\_VECTOR (3 downto 0);

b : in STD\_LOGIC\_VECTOR (3 downto 0); s : in STD\_LOGIC\_VECTOR (2 downto 0);

c : out STD\_LOGIC\_VECTOR (3 downto 0));

end abc;

architecture Behavioral of abc is begin


process (a,b,s) begin


case s is

when "000" => c <=a+ b; when "001" => c <=a - b; when "010" => c <= a and b; when "011" => c <= a or b;

when "100" => c <= a nand b; when "101" => c <= a nor b; when "110" => c <= not a; when "111" => c <= a;

when others => null; end case;

end process; end Behavioral;



LIBRARY ieee;

USE ieee.std\_logic\_1164.ALL;

-- Uncomment the following library declaration if using

-- arithmetic functions with Signed or Unsigned values

--USE ieee.numeric\_std.ALL;

ENTITY xyz IS

END xyz;

ARCHITECTURE behavior OF xyz IS

-- Component Declaration for the Unit Under Test (UUT)

COMPONENT abc

PORT(

a : IN std\_logic\_vector(3 downto 0);

b : IN std\_logic\_vector(3 downto 0); s : IN std\_logic\_vector(2 downto 0);

c : OUT std\_logic\_vector(3 downto 0)); END COMPONENT;

--Inputs

signal a : std\_logic\_vector(3 downto 0) := (others => '0'); signal b : std\_logic\_vector(3 downto 0) := (others => '0'); signal s : std\_logic\_vector(2 downto 0) := (others => '0');

--Outputs

signal c : std\_logic\_vector(3 downto 0);

-- No clocks detected in port list. Replace <clock> below with

-- appropriate port name

---constant <clock>\_period : time := 10 ns; BEGIN

-- Instantiate the Unit Under Test (UUT) uut: abc PORT MAP (

a => a,

b => b, s => s,

c => c );

-- Clock process definitions

-- <clock>\_process :process

-- begin

-- <clock> <= '0';

-- wait for <clock>\_period/2;

-- <clock> <= '1';

-- wait for <clock>\_period/2;

-- end process;

-- Stimulus process stim\_proc: process begin

-- hold reset state for 100 ns. wait for 100 ns;

a<="1010"; b<="1001"; s<="000";

wait for 100 ns;

a<="1010"; b<="1001"; s<="000";

wait for 100 ns; a<="1010"; b<="1001"; s<="001";

wait for 100 ns; a<="1010"; b<="1001"; s<="010";

wait for 100 ns; a<="1010"; b<="1001"; s<="101";

wait for 100 ns; a<="1010";

b<="1001"; s<="100";

wait for 100 ns; a<="1010"; b<="1001"; s<="101";

wait for 100 ns; a<="1010"; b<="1001"; s<="110";


wait for 100 ns; a<="1010"; b<="1001"; s<="111";

wait for 100 ns;

--- wait for <clock>\_period\*10;

-- insert stimulus here wait;

end process; END;



net a(3) loc=p96; net a(2) loc=p97; net a(1) loc=p100; net a(0) loc=p101; net b(3) loc=p90; net b(2) loc=p93; net b(1) loc=p94; net b(0) loc=p95; net s(2) loc=p85; net s(1) loc=p86; net s(0) loc=p87; net c(3) loc=p167; net c(2) loc=p166;

net c(1) loc=p165 net c(0) loc=p162;

Release 14.1 - xst P.15xf (nt64)

Copyright (c) 1995-2012 Xilinx, Inc. All rights reserved.

--> Parameter TMPDIR set to xst/projnav.tmp Total REAL time to Xst completion: 0.00 secs Total CPU time to Xst completion: 0.09 secs

--> Parameter xsthdpdir set to xst

Total REAL time to Xst completion: 0.00 secs Total CPU time to Xst completion: 0.09 secs

--> Reading design: abc.prj TABLE OF CONTENTS

1. Synthesis Options Summary
2. HDL Compilation
3. Design Hierarchy Analysis
4. HDL Analysis
5. HDL Synthesis
   1. HDL Synthesis Report
6. Advanced HDL Synthesis
   1. Advanced HDL Synthesis Report
7. Low Level Synthesis
8. Partition Report
9. Final Report
   1. Device utilization summary
   2. Partition Resource Summary
   3. TIMING REPORT

=========================================================================

\* Synthesis Options Summary \*

=========================================================================

|  |  |  |
| --- | --- | --- |
| ---- Source Parameters |  | |
| Input File Name |  | : "abc.prj" |
| Input Format |  | : mixed |
| Ignore Synthesis Constraint File | : NO |  |

---- Target Parameters

Output File Name : "abc"

Output Format : NGC

Target Device : xc3s400-5-pq208

---- Source Options

Top Module Name : abc

Automatic FSM Extraction : YES

FSM Encoding Algorithm : Auto

Safe Implementation : No

FSM Style : LUT

RAM Extraction : Yes

RAM Style : Auto

ROM Extraction : Yes

Mux Style : Auto

Decoder Extraction : YES Priority Encoder Extraction : Yes

Shift Register Extraction : YES

Logical Shifter Extraction : YES

XOR Collapsing : YES

ROM Style : Auto

Mux Extraction : Yes

Resource Sharing : YES

Asynchronous To Synchronous : NO

Multiplier Style : Auto

Automatic Register Balancing : No

|  |  |
| --- | --- |
| ---- Target Options  Add IO Buffers | : YES |
| Global Maximum Fanout | : 500 |
| Add Generic Clock Buffer(BUFG) | : 8 |
| Register Duplication | : YES |
| Slice Packing | : YES |
| Optimize Instantiated Primitives | : NO |
| Use Clock Enable | : Yes |
| Use Synchronous Set | : Yes |
| Use Synchronous Reset | : Yes |
| Pack IO Registers into IOBs | : Auto |
| Equivalent register Removal | : YES |

---- General Options

Optimization Goal : Speed

Optimization Effort 1

Keep Hierarchy : No

Netlist Hierarchy : As Optimized RTL Output : Yes

Global Optimization : All Clock Nets Read Cores : YES

Write Timing Constraints : NO

Cross Clock Analysis : NO

|  |  |
| --- | --- |
| Hierarchy Separator | : / |
| Bus Delimiter | : <> |
| Case Specifier | : Maintain |
| Slice Utilization Ratio | : 100 |
| BRAM Utilization Ratio | : 100 |
| Verilog 2001 | : YES |
| Auto BRAM Packing | : NO |
| Slice Utilization Ratio Delta | : 5 |

=========================================================================

=========================================================================

\* HDL Compilation \*

=========================================================================

Compiling vhdl file "D:/sakshiHAdder/bitalu/abc.vhd" in Library work. Entity <abc> compiled.

Entity <abc> (Architecture <behavioral>) compiled.

=========================================================================

\* Design Hierarchy Analysis \*

=========================================================================

Analyzing hierarchy for entity <abc> in library <work> (architecture <behavioral>).

=========================================================================

\* HDL Analysis \*

=========================================================================

Analyzing Entity <abc> in library <work> (Architecture <behavioral>). Entity <abc> analyzed. Unit <abc> generated.

=========================================================================

* HDL Synthesis \*

=========================================================================

Performing bidirectional port resolution...

Synthesizing Unit <abc>.

Related source file is "D:/sakshiHAdder/bitalu/abc.vhd". Found 4-bit 8-to-1 multiplexer for signal <c>.

Found 4-bit addsub for signal <c$addsub0000>. Summary:

inferred 1 Adder/Subtractor(s).

inferred 4 Multiplexer(s).

Unit <abc> synthesized.

INFO:Xst:1767 - HDL ADVISOR - Resource sharing has identified that some arithmetic operations in this design can share the same physical resources for reduced device utilization. For improved clock frequency you may try to disable resource sharing.

=========================================================================

HDL Synthesis Report Macro Statistics

# Adders/Subtractors 1

1. bit addsub 1

# Multiplexers 1

1. bit 8-to-1 multiplexer 1

=========================================================================

=========================================================================

* Advanced HDL Synthesis \*

=========================================================================

=========================================================================

Advanced HDL Synthesis Report Macro Statistics

# Adders/Subtractors 1

1. bit addsub 1

# Multiplexers 1

1. bit 8-to-1 multiplexer 1

=========================================================================

=========================================================================

* Low Level Synthesis \*

=========================================================================

Optimizing unit <abc> ... Mapping all equations...

Building and optimizing final netlist ...

Found area constraint ratio of 100 (+ 5) on block abc, actual ratio is 0. Final Macro Processing ...

=========================================================================

Final Register Report Found no macro

=========================================================================

=========================================================================

* Partition Report

\*=========================================================================

Partition Implementation Status

No Partitions were found in this design.

=========================================================================

* Final Report \*

=========================================================================

Final Results

RTL Top Level Output File Name : abc.ngr Top Level Output File Name : abc Output Format : NGC

Optimization Goal : Speed

Keep Hierarchy : No

Design Statistics

# IOs 15

|  |  |
| --- | --- |
| Cell Usage : |  |
| # BELS | : 34 |
| # LUT2 | : 5 |
| # LUT3 | : 10 |
| # LUT4 | : 6 |
| # MUXF5 | : 9 |
| # MUXF6 | : 4 |
| # IO Buffers | : 15 |
| # IBUF | : 11 |
| # OBUF | : 4 |

=========================================================================

Device utilization summary:

|  |  |  |  |
| --- | --- | --- | --- |
| Selected Device : 3s400pq208-5  Number of Slices: | 11 out of | 3584 | 0% |
| Number of 4 input LUTs: Number of IOs:  Number of bonded IOBs: | 21 out of  15  15 out of | 7168  141 | 0%  10% |

Partition Resource Summary:

No Partitions were found in this design.

========================================================================= TIMING REPORT

NOTE: THESE TIMING NUMBERS ARE ONLY A SYNTHESIS ESTIMATE.

FOR ACCURATE TIMING INFORMATION PLEASE REFER TO THE TRACE REPORT GENERATED AFTER PLACE-and-ROUTE.

Clock Information:

No clock signals found in this design Asynchronous Control Signals Information:

No asynchronous control signals found in this design Timing Summary:

Speed Grade: -5

Minimum period: No path found

Minimum input arrival time before clock: No path found Maximum output required time after clock: No path found Maximum combinational path delay: 12.624ns

Timing Detail:

All values displayed in nanoseconds (ns)

=========================================================================

Timing constraint: Default path analysis

Total number of paths / destination ports: 87 / 4

Delay: 12.624ns (Levels of Logic = 8) Source: s<0> (PAD)

Destination: c<3> (PAD)

Data Path: s<0> to c<3>

Gate Net

Cell:in->out fanout Delay Delay Logical Name (Net Name)

|  |  |  |  |
| --- | --- | --- | --- |
| IBUF:I->O | 14 | 0.715 | 1.179 s\_0\_IBUF (s\_0\_IBUF) |
| LUT3:I1->O | 3 | 0.479 | 0.771 c\_mux00001 (c\_mux00001) |

MUXF5:S->O 2 0.540 1.040 Maddsub\_c\_addsub0000\_cy<1>1\_f5 (Maddsub\_c\_addsub0000\_cy<1>)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| LUT4:I0->O | 1 | 0.479 | 0.740 | Maddsub\_c\_addsub0000\_xor<3>11\_SW0 (N2) |
| LUT3:I2->O | 1 | 0.479 | 0.000 | Maddsub\_c\_addsub0000\_xor<3>11 (c\_addsub0000<3>) |
| MUXF5:I0->O | 1 | 0.314 | 0.000 | Mmux\_c\_4\_f5\_2 (Mmux\_c\_4\_f53) |
| MUXF6:I0->O | 1 | 0.298 | 0.681 | Mmux\_c\_2\_f6\_2 (c\_3\_OBUF) |
| OBUF:I->O |  | 4.909 |  | c\_3\_OBUF (c<3>) |

Total 12.624ns (8.213ns logic, 4.411ns route) (65.1% logic, 34.9% route)

=========================================================================

Total REAL time to Xst completion: 4.00 secs Total CPU time to Xst completion: 4.22 secs

-->

Total memory usage is 4493160 kilobytes Number of errors : 0 ( 0 filtered) Number of warnings : 0 ( 0 filtered) Number of infos : 1 ( 0 filtered)